<!--This work is licensed under a Creative Commons Attribution-ShareAlike 4.0 International License (CC BY-SA) with Design Exception 1.0-->
<eagle version="7.1.0">
<drawing>
<library>
<packages>
<package name="QFN50P500X500X90-33N">
</package>
</packages>
<symbols>
<symbol name="NRF905">
<pin name="TRX_CE" direction="in"/>
<pin name="PWR_UP" direction="in"/>
<pin name="UPCLK" direction="out"/>
<pin name="VDD" direction="pwr"/>
<pin name="VSS" direction="pwr"/>
<pin name="CD" direction="out"/>
<pin name="AM" direction="out"/>
<pin name="DR" direction="out"/>
<pin name="MISO" direction="out"/>
<pin name="MOSI" direction="in"/>
<pin name="SCK" direction="in" function="clk"/>
<pin name="!CSN" direction="in"/>
<pin name="XC1" direction="in"/>
<pin name="XC2" direction="out"/>
<pin name="VDD_PA" direction="pwr"/>
<pin name="ANT1" direction="pas"/>
<pin name="ANT2" direction="pas"/>
<pin name="IREF" direction="in"/>
<pin name="DVDD_1V2" direction="pwr"/>
<pin name="TX_EN" direction="in"/>
<pin name="EXP" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="NRF905" prefix="U">
<description>RF Transceiver GFSK 2.5V/3.3V 32-Pin QFN EP Tray &lt;a href="https://pricing.snapeda.com/parts/NRF905/Nordic%20Semiconductor/view-part?ref=eda"&gt;Check availability&lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="NRF905"/>
</gates>
<devices>
<device name="" package="QFN50P500X500X90-33N">
<connects>
<connect gate="G$1" pin="!CSN" pad="13"/>
<connect gate="G$1" pin="AM" pad="7"/>
<connect gate="G$1" pin="ANT1" pad="20"/>
<connect gate="G$1" pin="ANT2" pad="21"/>
<connect gate="G$1" pin="CD" pad="6"/>
<connect gate="G$1" pin="DR" pad="8"/>
<connect gate="G$1" pin="DVDD_1V2" pad="31"/>
<connect gate="G$1" pin="EXP" pad="33"/>
<connect gate="G$1" pin="IREF" pad="23"/>
<connect gate="G$1" pin="MISO" pad="10"/>
<connect gate="G$1" pin="MOSI" pad="11"/>
<connect gate="G$1" pin="PWR_UP" pad="2"/>
<connect gate="G$1" pin="SCK" pad="12"/>
<connect gate="G$1" pin="TRX_CE" pad="1"/>
<connect gate="G$1" pin="TX_EN" pad="32"/>
<connect gate="G$1" pin="UPCLK" pad="3"/>
<connect gate="G$1" pin="VDD" pad="4 17 25"/>
<connect gate="G$1" pin="VDD_PA" pad="19"/>
<connect gate="G$1" pin="VSS" pad="5 9 16 18 22 24 26 27 28 29 30"/>
<connect gate="G$1" pin="XC1" pad="14"/>
<connect gate="G$1" pin="XC2" pad="15"/>
</connects>
<technologies>
<technology name="">
<attribute name="MF" value="Nordic Semiconductor"/>
<attribute name="Description" value="
                        
                            IC RF TxRx Only General ISM &lt; 1GHz - 433MHz, 868MHz, 915MHz 32-VFQFN Exposed Pad
                        
                    "/>
<attribute name="Package" value="VFQFN-32 Nordic Semiconductor"/>
<attribute name="Price" value="None"/>
<attribute name="SnapEDA_Link" value="https://www.snapeda.com/parts/NRF905/Nordic+Semiconductor+ASA/view-part/?ref=snap"/>
<attribute name="MP" value="NRF905"/>
<attribute name="Availability" value="In Stock"/>
<attribute name="Check_prices" value="https://www.snapeda.com/parts/NRF905/Nordic+Semiconductor+ASA/view-part/?ref=eda"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
